**Logic and Accuracy Testing Protocols**

**What is Logic and Accuracy Testing?**  
Logic and Accuracy (L&A) Testing is a set of procedures performed to ensure there are no errors on ballots or ballot displays and that voting machines are properly programmed. These tests occur prior to every election.

**How Does Testing Work?**  
Each type of device is tested with different protocols and for specific purposes. For each piece of equipment, the steps listed below will be completed to ensure the voting system operates as expected. Certain tasks such as candidate name proofing have already been completed.

**Testing Processes**

Insert Picture(s) of your Equipment

**Ballot Marking Devices**

1. Ballot styles are loaded on the ballot marking device.
2. Verify the collection of contests and candidates are correct.
3. Make pre-determined selections on the ballot marking device then complete the ballot.
4. Review the printed ballot card to ensure it matches the on screen selections.
5. Compare results from the printed ballot card to the expected results to verify accuracy.
6. Repeat the process for each ballot marking device being used.

**Precinct and Central Count Scanners**

Insert Picture(s) of your Equipment

1. Insert pre-determined test ballots into the scanner to ensure that:
   1. There are no paper size or stock issues
   2. All ballot styles (collections of contests and candidates) can be counted by the scanner
   3. Error conditions, such as smudged ballots, ballots with marginal marks, ballots with over-voted contests, tears, etc., are outstacked or otherwise recorded for future review, and adjudication or replication by staff.
2. Tabulate the results from test ballots cast on the scanner and compare them to the expected results to verify accuracy.

*Note: This is why the test ballots are marked with a predefined set of choices.*

**The Tabulation System** is tested by aggregating results from each scanner into the system. Each scanner has a removable media that loads the results into the central tabulation system to be aggregated with the other scanners. These results are combined   
with the results from   
the central county   
scanners, to ensure all   
results are added up   
and reported correctly.

**The Election Night Reporting System** is not part of the voting system but is what displays the results to the public on the internet. It is tested by transferring results data from the tabulation system on a secure memory device and loading it into a separate   
computer to ensure   
the public display of   
results reflect what   
is in the Tabulation   
System.

Insert Picture(s) of your Equipment

Insert Picture(s) of your Equipment